LED Wireless Battery Uplight
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USER MANUAL

Thank you very much for choosing our product. For safety purpose, please read this manual carefully before your operation. This manual included installation and using information. Please install and operate it according to this manual.
Part 1 Product 

 Product introduction

This product is designed for indoor use. Suitable applications include wash or effect lighting for architectural, stage or nightclub applications. This product can also be installed for use in signage and advertising using the dynamic functions available with DMX512 control. Direct input of DMX512 signal allows the units to be controlled from any DMX512 controller. This product can be operated as a single unit or in multiple units for large applications. 

1.2 Technical Specifications

Voltage: AC100-240V, 50/60Hz

Power: 90W

Light Source:6X15W RGBWA+UV 6in1 ultra bright LED
Lifespan: around 50,000-100,000 hours

Control: DMX 512, 6/10 channels

Control mode: Wireless DMX,DMX 512, Cellphone APP control, Auto mode, Master/Slave, Sound active

Beam angle: 35 º 

Net Weight：2.5Kg
Size: 140X138X197mm
1.3 Fetures
2.4G wireless electronic switch: can turn ON or OFF 2.4G wireless by MENU. [image: image2.jpg]197MM





WIFI wireless electronic switch: can turn ON or OFF WIFI power by MENU.

WIFI Module restore factory Settings, the Mudule can be restored to factory Settings by MENU, choose the network again

Display: LED digital display.

1.3 Safety Warning

IMPORTANT:

ALWAYS READ THE USER MANUAL BEFORE OPERATION. PLEASE CONFIRM THAT THE POWER SUPPLY STATED ON THE PRODUCT IS THE SAME AS THE MAINS POWER SUPPLY IN YOUR AREA.

● This product must be installed by a qualified professional.
● Always operate the equipment as described in the user manual.
● A minimum distance of 0.5m must be maintained between the equipment and combustible surface.

● The product must always be placed in a well ventilated area.

● Always make sure that the equipment is installed securely.

● DO NOT stand close to the equipment and stare directly into the LED light source.

● Always disconnect the power supply before attempting and maintenance.

● Always make sure that the supporting structure is solid and can support the combined weight of the products.

● The earth wire must always be connected to the ground.

● Do not touch the power cables if your hands are wet.

ATTENTION:
● This product left the place of manufacture in perfect condition. In order to maintain this condition and for safe operation, the user must always follow the instructions and safety warnings described in this user manual.

● Avoid shaking or strong impacts to any part of the equipment.

● Make sure that all parts of the equipment are kept clean and free of dust.

● Always make sure that the power connections are connected correct and secure.

● If there is any malfunction of the equipment, contact your distributor immediately.

● When transferring the product, it is advisable to use the original packaging in which the product left the factory.

● Shields, lenses or ultraviolet screens shall be changed if they have become damaged to such an extent that their effectiveness is impaired.

● The lamp (LED) shall be changed if it has become damaged or thermally deformed.

Part 2 Installation
2.1 Mounting:

2.1-1 Hanging

The product can be mounted in a hanging position using the supporting bracket. The bracket should be secured to the mounting truss or structure using a standard mounting clamp. Please note that when hanging the unit a safety cable should also be used

.

2.1-2 Upright

The product can be mounted in an upright or sitting position using the supporting brackets.
NOTE:

The product can be mounted at any angle and in any position. It is possible to further adjust the angle of the product using the two adjustment knobs located on the side of the fixture.

2.2 Special construction for DMX connection.

☆ At last fixture, the DMX cable has to be terminated with a terminator to reduce signal errors. Solder a 120-ohm 1/4W resistor between pin 2(DMX-) and pin 3(DMX+) into a 3-pin XLR-plug and plug it in the DMX-output of the last fixture.

☆ If the controller is 5-pin output, it’s necessary to use an adaptor to transfer signal from 5-pin output to 3-pin XLR-plug or you can connect cables as following:

[image: image3.jpg]3-PIN TO 5-PIN CONRERSION CHART

Conductor 3 Pin Female (OQutput) 5 Pin Male (Input)
Ground/Shiele Pin 1 Pin 1
Data (-) signal Pin 2 Pin 2
Data (+) signal Pin 3 Pin 3

Not used Pin 4

Not used Pin 5





Part 3 Display Panel Operation
3.1 Display panel menu instruction
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[MENU] menu selection or return to previous menu.

[DOWN] press [DOWN] through the menu list to decrease/change the value of the current function.

[UP] press [UP] through the menu list to increase/change the value of the current function.

[ENTER] confirm & quit out current function setting.
3.2 Display panel operation instruction

	Menu
	Item 1
	Item 2

	Dmx512
	A001-A512
	

	Shows
	1.Auto Color
	(1-99）Adjust peed

	
	2.Auto Fade
	(1-99）Adjust peed

	
	3.Auto Sudden
	(1-99）Adjust peed

	
	4.Auto Strobe
	(1-99）Adjust peed

	
	5.Wifi Mode
	

	Sound
	1.Sound Mode1
	(1-100）Adjust sound sensetivity

	
	2.Sound Mode2
	(1-100）Adjust sound sensetivity

	
	3.Sound Mode3
	(1-100）Adjust sound sensetivity

	
	4.Sound Mode4
	(1-100）Adjust sound sensetivity

	Color
	1.Custom Color
	R:0-255

	
	
	G:0-255

	
	
	B:0-255

	
	
	W:0-255

	
	
	A:0-255

	
	
	U:0-255

	
	2.Static Color
	01-32

	Set
	1.Dmx channel
	6CH/10CH

	
	2.2.4g wireless
	ON/OFF

	
	3.Infrarrd
	ON/OFF

	
	4.Display backlight
	0-100％

	
	5.Lcd Close time
	1. Open

	
	
	5S

	
	
	10S

	
	
	15S

	
	
	30S

	
	6.Fan speed
	1. Auto speed

	
	
	2. Slow speed

	
	
	Middle speed

	
	
	Fast speed

	
	7.Restore factory
	Passward

	
	8.MANUAL
	Passward

	
	9.Temperature
	ON/OFF

	
	10.Battery
	ON/OFF

	
	11.Background Color
	0-8

	Help
	Name
	6 Color

	
	Version
	V4.6

	
	DMX Channel
	10CH

	
	Run Time
	XXX

	
	User Time
	XXX

	
	Temperature
	XX ℃


3.3 DMX Channel instruction

	6CH
	10CH
	DMX Value
	Function Instruction

	
	CH1
	0~255
	Dimmer,the ninth channel(0~9)

	CH1
	CH2
	0~255
	Red dimming

	CH2
	CH3
	0~255
	Green dimming

	CH3
	CH4
	0~255
	Blue dimming

	CH4
	CH5
	0~255
	White dimming

	CH5
	CH6
	0~255
	Amber dimming

	CH6
	CH7
	0~255
	UV dimming

	
	CH8
	0~255
	Strobe from slow to fast

	
	CH9
	0~8
	OFF

	
	
	9-50  
	Static color mode (32 colors)

	
	
	51-100  
	Color change mode

	
	
	101-150  
	Color Pulse mode

	
	
	151-200  
	Color Fade mode 

	
	
	201-220  
	Sound mode 1

	
	
	221-240  
	Sound mode 2

	
	
	241-255  
	Sound mode 3

	
	CH10
	0-255
	This Channel depends on the value of the Ninth channel

1. The value of the 9 channel is 9-50, this channel is for color selection

2. The value of the 9 channel is 51-200, this channel is for speed adjustment(0 is the slowest, 255 is the fastest)


3.4 Smartphone App control

WIFI setting

Pls down load the LED LAMP APP by the QR code below:
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WIFI Setting: Open mobile WIFI Settings page, click the name of “LEDxxx " WLAN links, 

After the success linking, please open LED LAMP App,Choose the “LED LIGHT” to control the product.When WiFi signal receiving accident interrupt or cannot control, please exit the APP then reopen it.
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Part 4 Maintenance

The cleaning of internal must be carried out periodically to optimize light output. Cleaning frequency depends on the environment in which the fixture operates: damp, smoky or particularly dirty surrounding can cause greater accumulation of dirt on the fixture’s optics.

● Clean with soft cloth using normal glass cleaning fluid.

● Always dry the parts carefully.

● Clean the external optics at least every 20 days. 

● Clean the internal optics at least every 30/60 days – Up to vary products. 
Please ask professional technical to clean waterproof products and make sure the fixture will be reassembled well for waterproof.     
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